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直流水泵房外阀门井重建采购文件

Reconstruction of Valve Shaft Outside the Direct-flow

         Pump House Procurement file
我司位于印尼巴淡的中国华电科工集团有限公司印尼巴淡2x65mw燃煤电厂，拟开展直流水泵房外阀门井重建采购，现将采购说明如下。

Our company located in Batam, Indonesia 2x65MW coal-fired power plant of China Huadian Engineering Co., LTD. plans toReconstruction of Valve Shaft Outside the Direct-flow Pump House procurement. Now procurement is explained as follows.

一、采购项目概况

Overview of the Procurement Project

	1．项目/标段名称：

Project/Section name:
	直流水泵房外阀门井重建

Reconstruction of Valve Shaft Outside the Direct-flow Pump House

	2．采购人：
Purchaser: 
	PT.TJK POWER

	3．到货期限/服务期限：

Delivery time/service term:
	合同签订日后20天完成
20 days after contract signed

	4．到货地点/服务地点：

Delivery place/service place:
	印尼巴淡电厂
Batam power plant

	5．项目简介：

Project Introduction:
	循环水泵房门前有一处阀门井，原墙面有一部分用钢管作为支撑，经过雨水常年的浸泡，已全部腐蚀锈烂，如不修建，会影响设备的正常运行。

There is a valve shaft in front of the circulating pump room. Part of the original wall was supported by steel pipes, but after years of rainwater immersion, it has completely corroded and rusted. If not repaired, it will affect the normal operation of the equipment.

	6．采购范围：

Scope of Procurement:
	旧钢管及砼墙面拆除、基础清理、水泥垫层（100mm厚）、混凝土墙面（K300）、电缆沟处理。Demolition of old steel pipes and concrete walls, foundation cleaning, cement bedding (100mm thick), concrete walls (K300), and cable trench treatment.

	7. 是否设置最高限价（如设置，需标明限价金额）：

Whether to set a maximum price (if so, indicate the amount of the maximum price):
	否NO


二、资格审查方式及资格条件

Qualification examination method and qualification conditions

本次资格审查采用资格后审方式。合格的供应商应具有圆满履行合同的资格和能力，开启报价后将会首先对供应商进行资格审查，本次采购供应商必须同时具备以下资格要求。

This qualification review adopts the post-qualification review method. Qualified suppliers should have the qualification and ability to fulfill the contract satisfactorily. After opening the quotation, suppliers will be first qualified. Suppliers for this procurement must meet the following qualification requirements at the same time.

1. 资质要求：

（1）投标人为印尼境内合法注册的独立法人或其他组织，具有承担民事责任能力，具有订立合同的权利;

（2）投标人应提供符合印尼国家规定的可实施相应工程或服务的资质文件。
2. 信誉要求：

（1）没有被PT.TJK POWER列为D级供应商或纳入不良行为供应商管理，取消交易资格的；

（2）没有在中国华电科工集团有限公司及所属单位组织的采购和合同执行中被发现存在弄虚作假、围串标、拒绝签约、合同履约过程中发生供应商负主要责任的一般及以上安全质量事故及其他违法、违约行为且处理期未满的；

3. 不接受联合体响应；

4. 不存在下列情形之一：

（1）不同单位法定代表人、股东会成员、监事会成员或高管为同一人的（如某单位法定代表人为另一单位的监事）；母子公司或存在管理关系的不同单位同时报价；属于同一母公司的子公司或控股公司同时报价；

（2）被责令停业的,财产被接管或冻结的或其他丧失履约能力的情形；

（3）在最近三年内（报价截止日前）有骗取成交或严重违约或重大产品、工程质量问题的。

1. Qualifications:

(1) The bidder shall be an independent legal person or other organization legally registered in Indonesia, with the ability to bear civil liability and the right to conclude the contract;
(2) The bidder shall provide the qualification documents that are in line with the national regulations of Indonesia and can implement the corresponding project or service.
2. Credit requirements:

(1) Those who are not listed as D-level suppliers or included in the management of suppliers with bad behaviors by PT.TJK POWER, and whose trading qualification is revoked;

(2) No instances of fraud, bid rigging, refusal to sign contracts, general or above-level safety and quality incidents where suppliers bear primary responsibility during contract performance, or other illegal or breach-of-contract behaviors discovered in procurement activities and contract execution organized by China Huadian Science & Technology Group Co., Ltd. and its affiliated units that have not yet been resolved;

3. Unacceptability of consortium response;

4. None of the following circumstances exists:

(1) The legal representative, shareholders meeting members, board of supervisors members or senior executives of different units are the same person (for example, the legal representative of one unit is the supervisor of another unit); the parent company and subsidiary or different units with management relationship quote at the same time; the subsidiaries or holding companies of the same parent company quote at the same time;

(2) the business is ordered to suspend, the property is taken over or frozen, or other circumstances in which the business ability to perform is lost;

(3) Having defrauded the transaction, committed serious breach of contract or major product and project quality problems within the last three years (before the deadline for quotation).

三、评审小组及评审方法

Review Panel and review methodology
1. 本次采购的评审小组由采购人组建。

The review panel for this procurement shall be established by the purchaser.
2. 本次评审采用经评审的最低价法。

The evaluated lowest price method was used in this evaluation.

四、合同条款及格式

Contract Terms and Format

见附件：合同草稿。
See annex: draft contract.

五、技术规范书/服务范围要求

Technical specification/service scope requirements
（一）施工准备

1.人员准:组成施工队伍，明确各人员分工和责任:

2.设备准备:准备混凝土搅拌机、混凝土泵等必要施工设备:

3.材料准备:采购符合标准的混凝土、钢筋等施工材料:

4.现场准备:清理施工现场，确保施工场地平整、无障碍。

（二）施工工艺

5.模板搭建:根据设计要求搭建阀门井的模板，注意模板的平整和牢固:

6.钢筋安装:按照设计要求，在模板内设置预埋钢筋，注意钢筋的数量和位置:

7.混凝土浇筑:采用机械搅拌的方式，将混凝土均匀浇入模板内，确保浇筑质量均匀、

密实

8.养护处理:混凝土浇筑完成后，进行养护处理，保持水湿，防止裂缝的产生:

9.拆模验收:混凝土达到设计强度后，折除模板，进行验收，保证施工质量符合要求。

（三）质量控制

10.施工过程中严格按照设计要求执行:

11.严格控制混凝土的配比、搅拌时间等参数，确保混凝土后量符合标准；
12.钢筋的安装要符合相关规范，保证钢筋连接牢固:

13.施工现场要保持清洁，防止杂物掺入混凝土中:

14.在养护期间，按照要求进行养护处理，防止混凝土强度不足。

（四）工程量清单

	序号NO.
	项目名称

ITEM
	单位UNIT
	数量QUANTITY

	1
	旧钢管及砼墙面拆除

Demolition of old steel pipes and concrete walls
	m²
	24

	2
	基础清理

Basic cleanup
	m³
	2

	3
	水泥垫层（100mm厚）

Cement bedding (100mm thick)
	m³
	1

	4
	钢筋Φ13（@150m）

Reinforced steel Φ13 (at 150m intervals)
	kg
	1250

	5
	混凝土K300

Concrete K300
	m³
	12

	6
	电缆沟处理

cable trench treatment
	m³
	1


（I） Construction Preparation 

1.Personnel Allocation: Assemble a construction team with clearly defined roles and responsibilities for each member.

2. Equipment preparation: Prepare necessary construction equipment such as concrete mixer and concrete pump.

3. Material preparation: Procure construction materials including concrete and steel bars that meet the required standards.

4. Site preparation: Clear the construction site to ensure it is level and free of obstacles.

（II）Construction Techniques 

5. Formwork Installation: Construct the formwork for the valve shaft according to design specifications, ensuring both smoothness and structural integrity.

6. Reinforcement installation: Install embedded reinforcement bars within the formwork as per design specifications, ensuring correct quantity and positioning.

7. Concrete pouring: Use mechanical mixing to pour concrete uniformly into the formwork, ensuring consistent and dense quality.

 8. Curing process: After pouring, apply curing treatment to maintain moisture and prevent cracking.

9. Formwork Removal and Acceptance: Once the concrete reaches the designed strength, the formwork is removed and inspected to ensure construction quality meets the requirements.

（III） Quality Control 

10. Strictly follow the design specifications during construction:

11. Strictly control concrete mix proportions, mixing duration, and other parameters to ensure the final concrete quality meets standards; 12. Reinforcement installation must comply with relevant specifications to ensure secure connections:

13. The construction site must be kept clean to prevent debris from mixing into the concrete.

14. During the curing period, perform curing as required to prevent insufficient concrete strength.

（IV）Bill of quantities

	序号NO.
	项目名称

ITEM
	单位UNIT
	数量QUANTITY

	1
	旧钢管及砼墙面拆除

Demolition of old steel pipes and concrete walls
	m²
	24

	2
	基础清理

Basic cleanup
	m³
	2

	3
	水泥垫层（100mm厚）

Cement bedding (100mm thick)
	m³
	1

	4
	钢筋Φ13（@150m）

Reinforced steel Φ13 (at 150m intervals)
	kg
	1250

	5
	混凝土K300

Concrete K300
	m³
	12

	6
	电缆沟处理

cable trench treatment
	m³
	1


六、应答文件的提交

Submission of response documents

1. 请贵司于2026年3月18日24:00前，通过TJK公司网站提交应答文件，网址为： https://tjkpower.com。如有未尽事宜，请与我司联系人联系沟通。

2. 供应商应分项报价，报价应含税金，并列名税率和金额。

3. 采购人设有最高报价限价的，供应商的报价不得超过最高报价限价。
4. 除另有规定外，报价有效期为60天。

5.  在报价有效期内，供应商撤销响应（报价）文件的，应承担采购文件和法律规定的责任。

6. 出现特殊情况需要延长报价有效期的，采购人以书面形式通知供应商延长报价有效期。供应商应予以书面答复，同意延长的，不得要求或被允许修改其响应（报价）文件；供应商拒绝延长的，其报价失效。

1. Please submit the quotation materials to our dedicated procurement use the website https://tjkpower.situsdesain.com before 24:00 on March 18, 2026. For any remaining matters, please contact our designated contact person for further communication.

2. The supplier shall quote by item, including tax, and list the tax rate and amount.

3. If the purchaser has a maximum price limit, the suppliers quotation shall not exceed the maximum price limit.
4. Unless otherwise specified, the offer is valid for 60 days.

5. If the supplier revokes the response (offer) document within the validity period of the offer, it shall bear the liability stipulated in the procurement documents and laws.

6. If special circumstances require extension of the quotation validity period, the purchaser shall notify the supplier in writing to extend the quotation validity period. The supplier shall provide a written response. If the supplier agrees to the extension, it shall not be required or permitted to modify its response (quotation) documents; if the supplier refuses to extend, its quotation shall become invalid.

七、资格审查资料

Qualification review materials
除另有规定外，供应商应按下列规定提供资格审查资料，以证明其满足第二条规定的资质、信誉等要求。

Unless otherwise provided, the supplier shall provide qualification review materials in accordance with the following provisions to prove that it meets the qualification, financial, performance, reputation and other requirements specified in Article 2.

八、签订合同

CONTRACTING
采购人和成交供应商应当在成交通知书发出之日起30日内，根据采购文件、成交供应商的响应（报价）文件以及达成一致意见的技术要求、商务条件和价格订立书面合同，合同签订和（或）履行（包括但不限于实施/施工/服务、结算、开票）等事宜请跟采购人商务联系人联系。成交供应商无正当理由拒签合同，在签订合同时向采购人提出附加条件，采购人有权取消其成交资格。

The purchaser and the successful supplier shall execute a written contract within 30 days from the date of issuance of the Transaction Notice, based on the procurement documents, the successful suppliers response (quotation) documents, and mutually agreed technical requirements, commercial terms, and pricing. For matters including contract execution and/or performance (such as implementation/construction/service delivery, settlement, invoicing), please contact the purchasers designated business representative. If the successful supplier unreasonably refuses to sign the contract or imposes additional conditions during signing, the purchaser reserves the right to revoke its qualification as the successful bidder.
TJK POWER联系人及监督人员：

TJK POWER contact and supervisor:
联系人Contacts：刘署光
电话Telephone：(+62)778 - 807 0196  
电子邮件E-mail：Procurement.tjk@gmail.com  
监督人Supervisor：BAIHAQI
电话Telephone：+6281310115330
电子邮件E-mail：baihaqi.basyarah@gmail.com
附件1，报价书：

报价书
PT.TJK POWER：

我司研究了采购文件，愿意遵照询价文件全部内容。我们的投标总价为（大写）_________（币种）元，分项明细如下：

	序号
	项目名称
	单位
	数量
	单价
	合价

	1
	旧钢管及砼墙面拆除

Demolition of old steel pipes and concrete walls
	m²
	24
	
	

	2
	基础清理

Basic cleanup
	m³
	2
	
	

	3
	水泥垫层（100mm厚）

Cement bedding (100mm thick)
	m³
	1
	
	

	4
	钢筋Φ13（@150m）

Reinforced steel Φ13 (at 150m intervals)
	kg
	1250
	
	

	5
	混凝土K300

Concrete K300
	m³
	12
	
	

	6
	电缆沟处理

cable trench treatment
	m³
	1
	
	

	7
	
	
	
	含税总计

Total amount include tax
	


上述报价是为完成本项目的全部报价，我司承诺除此报价以外不会再向贵司要求任何费用的支付。

投标单位（公章）

投标单位法定代表人（签字）

投标单位地址_______________________

投标单位开户银行及账号______________

投标单位传真号_____________________

投标单位电话_______________________

投标单位邮编_______________________

日      期：        年    月    日


附件：（相应材料及说明）
Annex 1, quotation:

Offer letter
PT.TJK POWER：
We have studied the procurement documents and are willing to comply with all the contents of the inquiry documents. Our total bid price is (in words) _________ (currency), and the details are as follows:
	序号
	项目名称
	单位
	数量
	单价
	合价

	1
	旧钢管及砼墙面拆除

Demolition of old steel pipes and concrete walls
	m²
	24
	
	

	2
	基础清理

Basic cleanup
	m³
	2
	
	

	3
	水泥垫层（100mm厚）

Cement bedding (100mm thick)
	m³
	1
	
	

	4
	钢筋Φ13（@150m）

Reinforced steel Φ13 (at 150m intervals)
	kg
	1250
	
	

	5
	混凝土K300

Concrete K300
	m³
	12
	
	

	6
	电缆沟处理

cable trench treatment
	m³
	1
	
	

	7
	
	
	
	含税总计

Total amount include tax
	


The above quotation is for the completion of the project. Our company promises not to ask for any payment from your company except this quotation.

Tenderer (seal)：

Legal representative of the tenderer (signature)：

Address of the bidder_______________________

The bank and account number of the tenderer ______________

Fax number of the bidder _____________________

Bidders telephone _______________________

Bidders postal code _______________________

Date:


Appendix:(corresponding materials and instructions)

附件2，授权委托书:
授权委托书

本授权委托书声明：我司现授权委托我公司的下述代理人，以本公司的名义参加                                        （拟响应采购项目名称)的响应活动，此代理人在递交应答文件、报价、评审、合同谈判过程中所签署的一切文件和处理与之有关的一切事务，我均予以承认。

代理人无转委托权。

特此委托。

	代理人：
	
	性  别：
	

	单  位： 
	
	部  门：
	

	职  务：
	
	电  话：
	

	邮  箱：
	
	
	


法定代表人：（签字盖章）

代理人：（签字）

日  期：        年    月    日

Appendix 2, Power of Attorney:
letter of attorney

This power of attorney states: Our company hereby authorizes the following agent of our company to participate in the response activities (name of the proposed procurement project) in the name of our company. I acknowledge all documents signed by this agent during the submission of response documents, quotation, evaluation and contract negotiation, as well as all matters related to it.

The agent has no right of subdelegation.

I hereby entrust.

	Agent：
	
	Gender：
	

	Company： 
	
	Department：
	

	Function：
	
	Telephone：
	

	E-mail：
	
	
	


Legal representative:(signature and seal)

Agent:(signature)

Date:
3

