[image: image1.jpg], PEEEREA LT

CHINAHUADIAN CORPORATION

PEEHETE(REA)HRAS

CHINA HUADIAN ENGINEERING CO., LTD.



[image: image1.jpg]



#1、#2PT小室及工程师站通道地面瓷砖更换

采购文件

Procurement documents for #1 、#2 PT Chamber and Engineer Station Access way Floor Tile Replacement
我司位于印尼巴淡的中国华电科工集团有限公司印尼巴淡2x65mw燃煤电厂，拟开展#1、#2PT小室及工程师站通道地面瓷砖更换采购，现将采购说明如下。

Our company located in Batam, Indonesia 2x65MW coal-fired power plant of China Huadian Engineering Co., LTD. plans to Preparation of #1 、 #2 PT Chamber and Engineer Station Accessway Floor Tile Replacement ，Now procurement is explained as follows.

一、采购项目概况

Overview of the Procurement Project

	1．项目/标段名称：

Project/Section name:
	#1、#2PT小室及工程师站通道地面瓷砖更换

#1、#2 PT Chamber and Engineer Station Access way Floor Tile Replacement

	2．采购人：
Purchaser: 
	PT.TJK POWER

	3．到货期限/服务期限：

Delivery time/service term:
	合同签订后30日

Within 30 days after the contract is signed

	4．到货地点/服务地点：

Delivery place/service place:
	PT.TJK POWER

	5．项目简介：

Project Introduction:
	1、拆除原地面旧瓷砖

   Remove the existing floor tiles.
2、地面重新铺设瓷砖。

Replace the floor tiles.

	6．采购范围：

Scope of Procurement:
	拆除原地面旧瓷砖、铺设新瓷砖                                                       Remove the existing floor tiles and lay new tiles.

	7. 是否设置最高限价（如设置，需标明限价金额）：

Whether to set a maximum price (if so, indicate the amount of the maximum price):
	否NO


二、资格审查方式及资格条件

Qualification examination method and qualification conditions

本次资格审查采用资格后审方式。合格的供应商应具有圆满履行合同的资格和能力，开启报价后将会首先对供应商进行资格审查，本次采购供应商必须同时具备以下资格要求。

This qualification review adopts the post-qualification review method. Qualified suppliers should have the qualification and ability to fulfill the contract satisfactorily. After opening the quotation, suppliers will be first qualified. Suppliers for this procurement must meet the following qualification requirements at the same time.

1. 资质要求：

（1）投标人为印尼境内合法注册的独立法人或其他组织，具有承担民事责任能力，具有订立合同的权利;

（2）投标人应提供符合印尼国家规定的可实施相应工程或服务的资质文件。
2. 信誉要求：

（1）没有被PT.TJK POWER列为D级供应商或纳入不良行为供应商管理，取消交易资格的；

（2）没有在中国华电科工集团有限公司及所属单位组织的采购和合同执行中被发现存在弄虚作假、围串标、拒绝签约、合同履约过程中发生供应商负主要责任的一般及以上安全质量事故及其他违法、违约行为且处理期未满的；

3. 不接受联合体响应；

4. 不存在下列情形之一：

（1）不同单位法定代表人、股东会成员、监事会成员或高管为同一人的（如某单位法定代表人为另一单位的监事）；母子公司或存在管理关系的不同单位同时报价；属于同一母公司的子公司或控股公司同时报价；

（2）被责令停业的,财产被接管或冻结的或其他丧失履约能力的情形；

（3）在最近三年内（报价截止日前）有骗取成交或严重违约或重大产品、工程质量问题的。

1. Qualifications:

(1) The bidder shall be an independent legal person or other organization legally registered in Indonesia, with the ability to bear civil liability and the right to conclude the contract;
(2) The bidder shall provide the qualification documents that are in line with the national regulations of Indonesia and can implement the corresponding project or service.
2. Credit requirements:

(1) Those who are not listed as D-level suppliers or included in the management of suppliers with bad behaviors by PT.TJK POWER, and whose trading qualification is revoked;

(2) No instances of fraud, bid rigging, refusal to sign contracts, general or above-level safety and quality incidents where suppliers bear primary responsibility during contract performance, or other illegal or breach-of-contract behaviors discovered in procurement activities and contract execution organized by China Huadian Science & Technology Group Co., Ltd. and its affiliated units that have not yet been resolved;

3. Unacceptability of consortium response;

4. None of the following circumstances exists:

(1) The legal representative, shareholders meeting members, board of supervisors members or senior executives of different units are the same person (for example, the legal representative of one unit is the supervisor of another unit); the parent company and subsidiary or different units with management relationship quote at the same time; the subsidiaries or holding companies of the same parent company quote at the same time;

(2) the business is ordered to suspend, the property is taken over or frozen, or other circumstances in which the business ability to perform is lost;

(3) Having defrauded the transaction, committed serious breach of contract or major product and project quality problems within the last three years (before the deadline for quotation).

三、评审小组及评审方法

Review Panel and review methodology
1. 本次采购的评审小组由采购人组建。

The review panel for this procurement shall be established by the purchaser.
2. 本次评审采用经评审的最低价法。

The evaluated lowest price method was used in this evaluation.

若评标结果排序第二名的投标单位报价超过第一名报价10%及以上的，或第二名报价超过采购估算价的，不推荐备选预中标单位；若评标结果有效投标人数量仅剩两家，则不推荐备选预中标单位。

If the bid price of the bidder ranked second in the bid evaluation results exceeds the bid price of the first-ranked bidder by 10% or more, or if the second-ranked bid price exceeds the estimated procurement amount, no recommended candidate for pre-winning shall be recommended; if only two valid bidders remain after the bid evaluation process, no recommended candidate for pre-winning shall be recommended.
四、合同条款及格式

Contract Terms and Format

见附件：合同草稿。
See annex: draft contract.

五、技术规范书/服务范围要求

Technical specification/service scope requirements
1. 工期要求/服务期限 

Construction period/Service period

30天Days

2. 技术标准/服务标准

Technical/service standards

根据图纸要求施工

Construction in accordance with the drawings

3. 技术要求/服务要求

Technical/service requirements

（1）工程量

Quantities

	序号

NO
	项目名称

Project Name
	单位

Unit
	数量

Qty
	备注

Remark

	1
	#1、#2PT小室地面破损瓷砖拆除
Removal of damaged floor tiles in PT Rooms #1 and #2.
	m2
	110
	材料乙供
Material Supp By B Party

规格600mmx600mm

瓷砖颜色为白色，瓷砖等级为4A

Tile color is white, tile grade is 4A

	2
	#1、#2PT小室地面瓷砖铺设
Installation of new floor tiles in PT Rooms #1 and #2.
	m2
	110
	

	3
	电子间8米通道旧瓷砖拆除

Removal of old tiles from an 8-meter-wide corridor in the electronic equipment room
	m2
	90
	

	4
	铺设新瓷砖

Install new tiles
	m2
	90
	


（2）技术要求

Technical requirements

1）准备工作：在安装前，需要确认瓷砖的规格、数量、颜色等是否符合要求，同时确认施工现场的地面是否平整。
2）基层处理：镶贴瓷砖或面砖的基层，一般都是抹1:3的水泥砂浆一层，厚度15MM左右，并要求将表面用木抹子搓毛，个别凸凹和缺棱掉角部分要先刷一遍1:4的107胶水溶液，然后用1:3水泥砂浆补平，每次修补厚度10MM以内为宜。
3）弹线定位：根据地面的宽度，弹出面砖定位的水平缝线。
4）润湿基层：在粘贴之前，要先把基层表面清扫干净，铲除地面的余浆、毛刺，然后洒水润湿地面，也可在施工的前一天将基层地面浇水，要浇匀、湿透、表面无水。
5）刮抹粘结灰浆：用齿形抹子直接把107胶水泥素浆刮抹到基层上，厚度控制在4～6mm。
6）瓷砖安装：手持瓷砖地面粘贴，此后用橡胶锤或拳头振击，待瓷砖接缝处溢出灰浆，至表面平整为止。
7）瓷砖割裂：瓷砖安装需要根据实际情况进行割裂，割裂时需要使用专业工具，按照现场实际要求进行割裂。
8）清洁和养护：在瓷砖安装完成后，需要使用清洁剂清洗瓷砖表面的残留胶水和灰尘，在彻底干燥后，可以进行瓷砖的养护工作。新铺瓷砖不能立即进行使用，需要等到瓷砖完全贴合地面，并经过一段时间的养护后再使用。养护的时间需要根据瓷砖环境温度和干燥程度来确定，在这段时间内需要保持地面的清洁、干燥，并保持室内通风。

1) Preparation: Before installation, it is necessary to confirm whether the specification, quantity and color of ceramic tiles meet the requirements, and confirm whether the foundation, wall and ground of the construction site are smooth. 

2) base treatment: with ceramic tile or brick of the base, is generally 1:3 cement mortar layer, thickness of 15MM, and requires the surface with wood wipe rub hair, individual convex concave and missing Angle part to brush again 1:4 107 cement solution, and then use 1:3 cement mortar flat, each repair thickness within 10MM is appropriate.

3) elastic line positioning: according to the width of the ground, the horizontal suture of the elastic brick positioning. 

4) moisten the base: before pasting, to clean the surface of the base, remove the wall and Yin Angle of the remaining pulp, burrs, and then sprinkle water wet the ground, can also be in the day before the construction of the base ground watering, to pour evenly, wet, the surface without water. 

5) scraping and adhesive cement paste: scrape 107 cement paste directly to the base with tooth plaster, and the thickness is controlled at 4~6mm. 

6) Ceramic tile installation: paste the handheld ceramic tile on the wall, and then strike with a rubber hammer or fist, until the ceramic tile seam overflow mortar, until the surface is flat. 

7) Ceramic tile separation: ceramic tile installation needs to be split according to the actual situation, when the split needs to use professional tools, and the separation according to the design drawings. 

8) Cleaning and maintenance: after the installation of ceramic tiles, it is necessary to use detergent to clean the residual glue and dust on the surface of the ceramic tiles. After thorough drying, the maintenance of ceramic tiles can be carried out. New shop ceramic tile cannot undertake the use of the step immediately, need to wait for ceramic tile to fit the ground completely, and use again after a period of maintenance. The time of maintenance needs to be determined according to the environmental temperature and dryness degree of ceramic tile, during this time, the ground needs to be kept clean, dry, and maintain indoor ventilation.

六、应答文件的提交

Submission of response documents

1. 请贵司通过TJK公司网站提交应答文件，网址为： https://tjkpower.com。如有未尽事宜，请与我司联系人联系沟通。

2. 供应商应分项报价，报价应含税金，并列名税率和金额。

3. 采购人设有最高报价限价的，供应商的报价不得超过最高报价限价。
4. 除另有规定外，报价有效期为60天。

5.  在报价有效期内，供应商撤销响应（报价）文件的，应承担采购文件和法律规定的责任。

6. 出现特殊情况需要延长报价有效期的，采购人以书面形式通知供应商延长报价有效期。供应商应予以书面答复，同意延长的，不得要求或被允许修改其响应（报价）文件；供应商拒绝延长的，其报价失效。

1. Please submit the quotation materials to our dedicated procurement use the website https://tjkpower.com, For any remaining matters, please contact our designated contact person for further communication.

2. The supplier shall quote by item, including tax, and list the tax rate and amount.

3. If the purchaser has a maximum price limit, the suppliers quotation shall not exceed the maximum price limit.
4. Unless otherwise specified, the offer is valid for 60 days.

5. If the supplier revokes the response (offer) document within the validity period of the offer, it shall bear the liability stipulated in the procurement documents and laws.

6. If special circumstances require extension of the quotation validity period, the purchaser shall notify the supplier in writing to extend the quotation validity period. The supplier shall provide a written response. If the supplier agrees to the extension, it shall not be required or permitted to modify its response (quotation) documents; if the supplier refuses to extend, its quotation shall become invalid.

七、资格审查资料

Qualification review materials
除另有规定外，供应商应按下列规定提供资格审查资料，以证明其满足第二条规定的资质、信誉等要求。

Unless otherwise provided, the supplier shall provide qualification review materials in accordance with the following provisions to prove that it meets the qualification, financial, performance, reputation and other requirements specified in Article 2.

八、签订合同

CONTRACTING
采购人和成交供应商应当在成交通知书发出之日起30日内，根据采购文件、成交供应商的响应（报价）文件以及达成一致意见的技术要求、商务条件和价格订立书面合同，合同签订和（或）履行（包括但不限于实施/施工/服务、结算、开票）等事宜请跟采购人商务联系人联系。成交供应商无正当理由拒签合同，在签订合同时向采购人提出附加条件，采购人有权取消其成交资格。

The purchaser and the successful supplier shall execute a written contract within 30 days from the date of issuance of the Transaction Notice, based on the procurement documents, the successful suppliers response (quotation) documents, and mutually agreed technical requirements, commercial terms, and pricing. For matters including contract execution and/or performance (such as implementation/construction/service delivery, settlement, invoicing), please contact the purchasers designated business representative. If the successful supplier unreasonably refuses to sign the contract or imposes additional conditions during signing, the purchaser reserves the right to revoke its qualification as the successful bidder.
TJK POWER联系人及监督人员：

TJK POWER contact and supervisor:
联系人Contacts：Liu shu guang
电话Telephone：(+62) 082283529525 
电子邮件E-mail：495853472@qq.com

监督人Supervisor：BAIHAQI
电话Telephone：+6281310115330
电子邮件E-mail：baihaqi.basyarah@gmail.com
附件1，报价书：

报价书

我司研究了采购文件，愿意遵照询价文件全部内容。我们的投标总价为（大写） _________ （印尼盾）元，分项明细如下：

上述报价是为完成本项目的全部报价，我司承诺除此报价以外不会再向贵司要求任何费用的支付。

投标单位（公章）

投标单位法定代表人（签字）

投标单位地址_______________________

投标单位开户银行及账号______________

投标单位传真号_____________________

投标单位电话_______________________

投标单位邮编_______________________

日      期：        年    月    日


附件：（相应材料及说明）
Annex 1, quotation:

Offer letter
PT.TJK POWER：
We have studied the procurement documents and are willing to comply with all the contents of the inquiry documents. Our total bid price is (in words) _________ (currency), and the details are as follows:
The above quotation is for the completion of the project. Our company promises not to ask for any payment from your company except this quotation.

Tenderer (seal)：

Legal representative of the tenderer (signature)：

Address of the bidder_______________________

The bank and account number of the tenderer ______________

Fax number of the bidder _____________________

Bidders telephone _______________________

Bidders postal code _______________________

Date:


Appendix:(corresponding materials and instructions)

附件2，授权委托书:
授权委托书

本授权委托书声明：我司现授权委托我公司的下述代理人，以本公司的名义参加                                        （拟响应采购项目名称)的响应活动，此代理人在递交应答文件、报价、评审、合同谈判过程中所签署的一切文件和处理与之有关的一切事务，我均予以承认。

代理人无转委托权。

特此委托。

	代理人：
	
	性  别：
	

	单  位： 
	
	部  门：
	

	职  务：
	
	电  话：
	

	邮  箱：
	
	
	


法定代表人：（签字盖章）

代理人：（签字）

日  期：        年    月    日

Appendix 2, Power of Attorney:
letter of attorney

This power of attorney states: Our company hereby authorizes the following agent of our company to participate in the response activities (name of the proposed procurement project) in the name of our company. I acknowledge all documents signed by this agent during the submission of response documents, quotation, evaluation and contract negotiation, as well as all matters related to it.

The agent has no right of subdelegation.

I hereby entrust.

	Agent：
	
	Gender：
	

	Company： 
	
	Department：
	

	Function：
	
	Telephone：
	

	E-mail：
	
	
	


Legal representative:(signature and seal)

Agent:(signature)

Date:
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